{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Canaleta de concreto polímero","Auxiliar"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Canaleta de concreto polímero","index":0,"n_rows":6,"n_cols":24,"rows_kept":6,"cut":false,"hidden":false,"merged":[[1,9,4,9],[1,13,1,19],[1,10,1,11],[0,0,0,19],[1,12,2,12]]}
["PLANILHA DE CÁLCULO  -  CANALETA BM"]
["km",null,"POSIÇÃO","ÁREA",null,"TEMPO  DE","INTENS.","VAZÃO","DECLIVI-","TIPO DE CANALETA","DIMENSÕES",null,"COMPRI-MENTO","DIMENSIONAMENTO"]
[null,null,null,"A","C","CONCEN-","PLUVIO-","Q","DADE",null,"b","h",null,"RUGOSIDADE","ÁREA","PERÍMETRO","RAIO ","VELOCIDADE","LÂMINA","RELAÇÃO",null,"H","Qesc","Qatingir"]
["INICIAL","FINAL","RELATIVA",null,null,"TRAÇÃO","MÉTRICA",null,"I",null,null,null,"L","DE MANNING","MOLHADA","MOLHADO","HIDRÁULICO",null,"Y","Y/H",null,null,"Manning","Racional"]
[null,null,null,"( ha )",null,"tc ( min. )","i ( mm/min. )","( m3/s )","( m/m )",null,"(m)","(m)","(m)",null,"( m² )","(m)","(m)","( m/s )","( m )",null,null,"( m)","( m³/s )","( m³/s )"]
[null,null,"L1",3.8319999999999999E-3,0.65,10,2.457869901627697,{"$f":"(D6*E6*G6)/6","v":1.020343725162378E-3},5.5991041433370664E-2,"HEXALINE",{"$f":"IFERROR((VLOOKUP(J6,Auxiliar!$E$4:$G$8,2,0)),\"-\")","v":8.7999999999999995E-2},{"$f":"IFERROR((VLOOKUP(J6,Auxiliar!$E$4:$G$8,3,0)),\"-\")","v":5.5E-2},11,1.0500000000000001E-2,{"$f":"IF(J6=\"SELF100 H9,5\",(0.3395*S6^2)+(0.0597*S6)-(0.0004),IF(J6=\"SLIMLINE\",(-0.2796*S6^2)+(0.1319*S6)-0.0015,IF(J6=\"HEXALINE\",((0.0521*S6^2)+(0.083*S6)-0.0002),0)))","v":1.4388354994132073E-3},{"$f":"IF(J6=\"SELF100 H9,5\",(-6.9498*S6^2)+(2.7921*S6)+0.0265,IF(J6=\"SLIMLINE\",(16.392*S6^2)+(0.4731*S6)+0.0889,IF(J6=\"HEXALINE\",((-2.0201*S6^2)+(2.1648*S6)+0.0624),0)))","v":0.10385832333927618},{"$f":"IFERROR((O6/P6),\"-\")","v":1.3853829458741914E-2},{"$f":"IFERROR(((Q6^(2/3))*(I6^0.5))/N6,\"-\")","v":1.299919718890272},{"$f":"V6","v":1.9506167949100702E-2},{"$f":"IFERROR(S6/L6,\"calcular\")","v":0.35465759907455824},null,1.9506167949100702E-2,{"$f":"IFERROR(R6*O6,\"-\")","v":1.8703706379265606E-3},{"$f":"H6","v":1.020343725162378E-3}]

{"sheet":"Auxiliar","index":1,"n_rows":6,"n_cols":9,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,"Canal ACO Monoblock","Base","Hútil","Am","Pm"]
[null,null,null,null,"SELF100 H9,5",9.8000000000000004E-2,0.08]
[null,null,null,null,"SLIMLINE",0.11,0.11]
[null,null,null,null,"HEXALINE",8.7999999999999995E-2,5.5E-2]